For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Turn the ignition OFF.
2. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.
3. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.

1 | Secondary Air Injection Pump Fastener (Qty: 2)

#### Procedure

1. Disconnect both quick connectors.
2. Disconnect the electrical connector.

Caution: Refer to Fastener Caution in the Preface section.

Tighten
17 N·m (13 lb ft)

2 | Secondary Air Injection Pump