For 1990-2009 cars

## Oil Level Indicator and Tube Removal LDK

1. Disconnect the knock sensor from the oil level indicator tube (1).
2. Remove the electrical wiring harness from the oil level indicator tube.
3. Remove the oil level indicator tube bracket to the intake manifold bolt.
4. Remove the oil level indicator (2) and the oil level indicator tube from the oil pan.
5. Inspect the O-rings for damage. Replace if damaged.