For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove left side luggage compartment trim. Refer to Rear Compartment Side Trim Panel Replacement.

1 | Electronic Suspension Front Position Sensor Fastener Tighten 9 N·m(80 lb in)
2 | Electronic Suspension Control Module Console

#### Procedure

Remove the bracket from the control module. Slide the control module down from the bracket.

3 | Electronic Suspension Control Module

#### Procedure

Disconnect the connectors.