For 1990-2009 cars

### Removal

1. Remove the transmission. Refer to Transmission Replacement.
2. Detach pressure line (1) from central release and unscrew bolt (2).
3. Remove connector for pressure line (1).

• | Remove retaining clip (2).

• | Remove connector.

• | Replace retaining clip in connector.

| Note: If necessary, bend squeeze together slightly.

4. Remove pressure line.

• | Clip pressure line out of fastening sleeve using a screwdriver or equivalent.

| Note: Carefully disengage retaining lugs.

• | Remove pressure line.

5. Remove fastening sleeve.

Note: Fastening sleeve must be replaced after removal.

• | Disengage fastening sleeve (1) from clutch housing.

• | Slide fastening sleeve upwards.

• | Remove fastening sleeve.

6. Check seal ring and pressure line for damage, replace if necessary.

### Installation

1. Attach fastening sleeve (1). Push into transmission housing - must noticeably engage.

Note: Insert projection on sleeve in the slot provided in the transmission.

2. Install pressure line (1) and insert in fastening sleeve - must noticeably engage.
3. Attach pressure line and tighten nut (2).
4. Attach connector for pressure line (1) and put connector on pressure line - retaining clip (2) must noticeably engage.
5. Install the transmission. Refer to Transmission Replacement.