For 1990-2009 cars

## Water Pump Pulley Replacement LDE/A16XER, 2H0/A18XER

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the power steering pump pulley belt, Refer to link.
2. Remove the drive belt. Refer to Drive Belt Replacement.

1 | Water Pump Pulley Fastener (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten X N·m (X lb in)
2 | Water Pump Pulley