For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the engine cover. Refer to Engine Cover Replacement
2. Disconnect the electrical connector.

1 | Exhaust Recirculation Valve solenoid fasteners (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 4.5 N·m(40 lb in)
2 | Vacuum hoses
3 | Exhaust Gas Recirculation Vacuum Regulator Solenoid Valve