For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the plenum water deflector. Refer to Plenum Water Deflector Replacement.

1 | Windshield Washer Nozzle Assembly

#### Procedure

1. Disconnect the windshield washer hose from the windshield washer nozzle.
2. Unclip the windshield washer nozzle from the bottom side in order to release it and then push it through the plenum water deflector to remove.