For 1990-2009 cars

#### Special Tools

• | EN 47981 Crankshaft Balancer Holding Tool

• | EN 956-1 Tool Extension

• | EN 47982 Crankshaft Balancer Remover

For equivalent regional tools, refer to Special Tools.

1. Install the EN 47981 holder (1) with EN 956-1 extension (2) to crankshaft balancer.
2. Remove the crankshaft balancer bolt (3).
3. Install the EN 47982 remover (1)
4. Remove the crankshaft balancer with EN 47982 remover .