For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the transmission. Refer to Transmission Replacement.
3. Disconnect the clutch actuator cylinder pipe from the clutch actuator cylinder. Refer to Clutch Actuator Cylinder Pipe Replacement.

1 | Clutch Actuator Cylinder Fastener (Qty: 3) Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

Use the appropriate thread sealant on the fasteners. Refer to Adhesives, Fluids, Lubricants, and Sealers for the appropriate sealant.

Tighten
20N·m (15 lb ft) plus 60 degrees

2 | Clutch Actuator Cylinder

#### Procedure

Bleed the clutch actuator cylinder before fitting the gearbox. Refer to Hydraulic Clutch Bleeding.