For 1990-2009 cars

Callout | Component Name
--- | ---
Warning: When a hood hold open device is being removed or installed, provide alternate support to avoid the possibility of damage to the vehicle or personal injury. Caution: Apply pressure only at the end of the liftgate/hood assist rod that you are removing or attaching. Do NOT apply pressure to the middle of the rod because damage or bending will result.
1 | Hood Open Assist Rod Retainer (Qty: 2)

#### Procedure

1. Release the locking tabs on the strut.
2. Ensure the clip is fully seated when the rod is reinstalled. If the clip cannot be fully seated a new rod should be installed.