For 1990-2009 cars

Warning: Bodily injury may occur if the cleaning solvent is inhaled or exposed to the skin.

1. Clean the piston oil nozzle in cleaning solvent using or equivalent. Refer to Adhesives, Fluids, Lubricants, and Sealers.

Warning: Wear safety glasses when using compressed air in order to prevent eye injury.

2. Dry the piston oil nozzle with compressed air.
3. Inspect the piston oil nozzle for the following:

• | For cracks or damage

• | Plugged oil passages (1)

• | Bent, misaligned or cracked oil nozzle tube (2)

• | Bent or broken clip (3)