For 1990-2009 cars

## Rear Axle Upper Control Arm Replacement GNE

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the rear tire and wheel assembly. Refer to Tire and Wheel Removal and Installation.

1 | Rear Suspension Upper Control Arm Inner Fastener Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

Torque on nut.

Tighten
150 N·m (111 lb ft)

2 | Rear Suspension Link Outer Fastener

#### Procedure

1. Install NEW bolt.
2. Torque on nut.

Tighten
115 N·m (85 lb ft) + 90 degrees + 15 degrees

3 | Rear Axle Upper Control Arm

#### Procedure

1. Remove cable harness clips from control arm.
2. Use a proper jack stand to load the knuckle when tightening the fasteners.
3. After installation, check the rear alignment. Refer to Wheel Alignment Measurement.

## Rear Axle Upper Control Arm Replacement GNC

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the rear tire and wheel assembly. Refer to Tire and Wheel Removal and Installation.

1 | Rear Axle Upper Control Arm Inner Fastener Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

Torque on nut.

Tighten
150 N·m (111 lb ft)

2 | Rear Axle Upper Control Arm Outer Fastener

#### Procedure

Torque on nut.

Tighten
115 N·m (X lb ft) + 90 degrees + 15 degrees

3 | Rear Axle Upper Control Arm