For 1990-2009 cars

## Exhaust Manifold Replacement Diesel

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the turbocharger. Refer to Turbocharger Replacement.
2. Remove fastener oil dipstick tube for access.

1 | Exhaust Manifold Fastener (Qty: 9) Caution: Refer to Fastener Caution in the Preface section. Tighten 20 N·m (15 lb ft)
2 | Exhaust Manifold Fastener Spacer (Qty: 9)
3 | Exhaust Manifold

#### Procedure

Transfer or replace the exhaust manifold gasket as needed.

## Exhaust Manifold Replacement LKD/A20NHT

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the turbocharger replacement. Refer to Turbocharger Replacement.
2. Remove the exhaust manifold heat shield. Refer to LINK.

1 | Exhaust Manifold Fastener (Qty: 10) Caution: Refer to Fastener Caution in the Preface section. Tighten X N·m (X lb ft)
2 | Exhaust Manifold