For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Disconnect the Battery Negative Terminal. Refer to Battery Negative Cable Disconnection and Connection
2. Disconnect the electrical connectors.

1 | Battery Cover

#### Procedure

1. Release Battery cover rear retainers
2. Lift upwards to release the battery cover front retainers.

2 | Glow Plug Control Module

#### Procedure

Release the Glow Plug Control Module Retainer and lift upwards.