For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

Remove the air cleaner assembly. Refer to Air Cleaner Assembly Replacement.

1 | Camshaft Position Actuator Solenoid Valve Fastener Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

Disconnect the electrical connector.

Tighten
10 N·m (89 lb in)

2 | Camshaft Position Actuator Solenoid Valve