For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove front seat head restraint. Refer to Front Seat Head Restraint Replacement.
2. Remove front seat head restraint adjust rod guide. Refer to Front Seat Head Restraint Adjust Rod Guide Replacement.

1 | Front Seat Head Restraint Adjust Rod Guide
2 | Front Seat Head Restraint Guide Bezel

#### Procedure

1. Position front seat head restraint guide bezel.
2. Attach front seat head restraint guide bezel at front seat head restraint adjust rod guide.

Tip
After removal of head restraint install both head restraint adjust rod guides.