For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the headlining trim panel. Refer to Headlining Trim Panel Replacement
2. Remove body lock pillar upper trim panel. Refer to Body Lock Pillar Upper Trim Panel Replacement
3. Remove rear compartment side trim panel. Refer to Rear Compartment Side Trim Panel Replacement

1 | Sunroof Housing Rear Drain Hose

#### Procedure

1. Remove the sunroof housing rear drain hose from the sunroof assembly.
2. Remove the rubber grommet from the tail lamp pocket.
3. Draw the rear drain hose out of the c-pillar.
4. Separate the rubber grommet from the rear drain hose.

Tip
It`s only necessary to lower the headlining trim panel in the rear area.