For 1990-2009 cars

## Parking Brake Rear Cable Replacement J71

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Release electric park brake.

1.1. | Set ignition in Run mode and put your foot on top of the service brake.

1.2. | Press park brake switch down and hold for 5 seconds, then a solid yellow telltale is shown on instrument panel.

1.3. | Press park brake switch again within 5 seconds, then a flashing yellow telltale is shown on instrument panel.

2. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
3. Remove the tire and wheel assembly. Refer to Tire and Wheel Removal and Installation.
4. Remove the rear wheelhouse panel liner. Refer to Rear Wheelhouse Panel Liner Replacement.

1 | Electric Park Brake Module Cable Caution: Refer to Fastener Caution in the Preface section. Tighten 6 N·m (53 lb in)
2 | Retainer Washer
3 | Park Brake Cable
4 | Protector Park Brake Cable
5 | Retainer Washer (Qty: 2)
6 | Park Brake Cable Assembly

## Parking Brake Rear Cable Replacement Manual

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the front floor console. Refer to Front Floor Console Replacement
2. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.

1 | Park Brake Cable Equalizer

#### Procedure

1. Carefully position the driveline tunnel insulator downward just enough to access the cable equalizer.
2. Remove the clip and disconnect the cables from the equalizer.

2 | Park Brake Cable

#### Procedure

Disconnect the park brake cables from the park brake actuator levers on the brake calipers.

3 | Park Brake Cable Retainer (Qty: 4)
4 | Parking Brake Rear Cable