For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

Remove the drive belt. Refer to Drive Belt Replacement.

1 | Drive Belt Idler Pulley Fastener Caution: Refer to Fastener Caution in the Preface section. Tighten X N·m (X lb ft)
2 | Drive Belt Idler Pulley
3 | Drive Belt Tensioner Fastener (Qty: 3) Tighten 25 N·m (19 lb ft)
4 | Drive Belt Tensioner Tip Remove the wiring harness retainer from the drive belt tensioner.