For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the ignition coil. Refer to Ignition Coil Replacement.
2. Remove the engine venting pipe.
3. Remove the positive crankcase ventilation pipe connector.

1 | Camshaft Cover Positive Crankcase Ventilation Pipe Connector
2 | Camshaft Cover Fastener (Qty: 11) Caution: Refer to Fastener Caution in the Preface section. Tighten X N·m (X lb in)
3 | Camshaft Cover