For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

Remove both front floor console extension panels. Refer to Front Floor Console Extension Panel Replacement.

1 | Ashtray
2 | Instrument Panel Ashtray Housing

#### Procedure

1. Use a flat-bladed plastic trim tool to release the I/P ashtray housing from the instrument panel.
2. Disconnect the electrical connections.
3. If replacing the I/P panel ashtray housing, transfer all necessary components.