For 1990-2009 cars

## Driver or Passenger Seat Side Inflatable Restraint Module Replacement 6-Way Hybrid, 6-Way Hybrid Sport

### Removal Procedures

Warning: Refer to SIR Warning in the Preface section.

1. 1. Disable the SIR System. Refer to SIR Disabling and Enabling.
2. Remove Driver or Passenger Seat. Refer to Driver or Passenger Seat Replacement.
3. Remove front seat outer adjuster finish cover. Refer to Driver or Passenger Seat Outer Adjuster Finish Cover Replacement.
4. Remove Driver or Passenger Seat Recliner Lever. Refer to Driver or Passenger Seat Recliner Lever Replacement.
5. Remove Tilt Adjuster Lever. Refer to Front Seat Tilt Adjuster Lever Replacement.
6. Remove Driver or Passenger Seat Adjuster Finish Cover. Refer to Driver or Passenger Seat Adjuster Finish Cover Replacement.
7. Remove Driver or Passenger Seat Inner Recliner Finish Cover. Refer to Driver or Passenger Seat Inner Recliner Finish Cover Replacement.
8. Remove Front Seat Head Restraint. Refer to Front Seat Head Restraint Replacement.
9. Remove Front Seat Head Restraint Guide Bezel. Refer to Front Seat Head Restraint Guide Bezel Replacement.
10. Remove the Front Seat Head Restraint Adjust Rod Guide. Refer to Front Seat Head Restraint Adjust Rod Guide Replacement.
11. Clip out Securing (1) of recliner control shaft (2).
12. Remove Recliner Control (1) from recliner shaft (2). Unhinge the cushion strap (3) at seat frame!

Note: For loosening move the cushion upper and pull from backrest frame.

13. Loose the front seat back cushion at backrest left side (1) and right side (2).
14. Clip out the front seat back cushion vent fan mat (3) of vent fan (4). Pull the cushion (5) in front to surface.
15. Loosen both nuts (1,2) from Seat Side Inflatable Restraint Module (3).
16. Disconnect the wiring harness connector (2) from Seat Side Inflatable Restraint Module (1).
17. Disconnect wiring harness connector (1) of the Seat Back Cushion Heater.
18. Remove Front Seat Back Cushion with cushion Pad (1) from backrest frame (2).
19. Install Seat Side Inflatable Restraint Module (1) out of the textile straps (2).
20. Install Seat Side Inflatable Restraint Module (1) at cushion cover with the textile straps (2).
21. Install Front Seat Back Cushion with cushion Pad (1) at the backrest frame (2).
22. Connect the wiring harness Connector (1) of the Seat Back Cushion Heater.

Note: Proof the correct locking of wiring harness connector (2),

23. Connect the wiring harness connector (2) from Seat Side Inflatable Restraint Module (1).

Caution: Refer to Fastener Caution in the Preface section.

24. Position Seat Side Inflatable Restraint Module (3) the backrest frame. Screw both nuts (1,2) from Seat Side Inflatable Restraint Module (3) and tighten to 3.25 N·m (29 lb in).
25. Clip in the Front Seat Back Cushion Vent Fan mat (3) at the vent fan (4). Position the cushion (5).
26. Install Front Seat Back Cushion at backrest Left Side (1) and Right Side (2).
27. Install the Front Seat Head Restraint Adjust Rod Guide. Refer to Front Seat Head Restraint Adjust Rod Guide Replacement.
28. Install the Front Seat Head Restraint Guide Bezel. Refer to Front Seat Head Restraint Guide Bezel Replacement.
29. Install the Front Seat Head Restraint. Refer to Front Seat Head Restraint Replacement.
30. Close the Cushion at backrest rear side.
31. Install the Driver or Passenger Seat Inner Recliner Finish Cover. Refer to Driver or Passenger Seat Inner Recliner Finish Cover Replacement.
32. Install the Driver or Passenger Seat Adjuster Finish Cover. Refer to Driver or Passenger Seat Adjuster Finish Cover Replacement.
33. Install the Tilt Adjuster Lever. Refer to Front Seat Tilt Adjuster Lever Replacement.
34. Install the Driver or Passenger Seat Recliner Lever. Refer to Driver or Passenger Seat Recliner Lever Replacement.
35. Install the front seat outer adjuster finish cover. Refer to Driver or Passenger Seat Outer Adjuster Finish Cover Replacement.
36. Remove Driver or Passenger Seat. Refer to Driver or Passenger Seat Replacement.