For 1990-2009 cars

## Radiator Inlet Hose Replacement Diesel

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Drain the cooling system. Refer to Cooling System Draining and Filling.
2. Remove the power steering fluid reservoir. Refer to Power Steering Fluid Reservoir Replacement.

1 | Radiator Inlet Hose

#### Procedure

1. Using a hose clamp tool, reposition the radiator inlet hose clamp and detach the hose from the radiator.
2. Using a hose clamp tool, reposition the radiator inlet hose clamp and detach the hose from the engine.
3. After installation, fill the cooling system. Refer to Cooling System Draining and Filling.
4. After repairs, inspect the cooling system for leaks.

## Radiator Inlet Hose Replacement LDK/A20NHT

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Drain the engine cooling fluid. Refer to Cooling System Draining and Filling.
2. Remove engine appearance cover replacement. Refer to LINK.
3. Remove the engine coolant air bleed hose. Refer to Engine Coolant Air Bleed Hose Replacement.

1 | Radiator Inlet Hose Retainer (Qty: 2)