For 1990-2009 cars

Callout | Component Name
--- | ---
Warning: When a hood hold open device is being removed or installed, provide alternate support to avoid the possibility of damage to the vehicle or personal injury.

#### Preliminary Procedure

Disconnect the hood strut. Refer to Hood Strut Replacement

1 | Hood Hinge Fastener (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 20 N·m (15 lb ft)
2 | Hood

#### Procedure

Transfer any parts as needed.