For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. If equipped, remove the Fuel Tank Heat Shield. Refer to Front Air Deflector Replacement
2. Disconnect the electrical connectors.

Warning: Gasoline or gasoline vapors are highly flammable. A fire could occur if an ignition source is present. Never drain or store gasoline or diesel fuel in an open container, due to the possibility of fire or explosion. Have a dry chemical (Class B) fire extinguisher nearby.

1 | Fuel Filter Assembly to Fuel Filter Bracket Retainer

#### Procedure

1. Release the Fuel Filter Assembly Retainer using a screwdriver.
2. Lift the Filter upwards to disengage the Fuel Filter for the Fuel Filter Bracket.

2 | Fuel Filter Assembly Inlet and Outlet pipe

#### Procedure

1. Release the Fuel pipes to the Fuel Filter Assembly (Qty: 2)
2. Pull the Fuel filter away from the Fuel Tank and downwards to remove from the Fuel Filter Bracket.

3 | Fuel Filter Assembly