For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Lift and support the vehicle. Refer to Lifting and Jacking the Vehicle.

1 | Front Bumper Valance Panel Retainer

#### Procedure

1. Release the seven flat locking retainers from the front bumper fascia.
2. Push the front bumper valance panel outward from the front bumper fascia in order to remove.

Tip
Using a small flat-bladed tool, pull and release the outer front bumper fascia locking retainer from the front bumper valance panel.

2 | Front Bumper Valance Panel