For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Disconnect battery. Refer to Link.
2. Drain the coolant. Refer to Link.
3. Remove the manifold exhaust. Refer to Link.
4. Remove the engine oil cooler pipe. Refer to Link.

1 | Engine Oil Cooler Housing Fastener (Qty: 5) Caution: Refer to Fastener Caution in the Preface section. Tighten X N·m (X lb in)
2 | Engine Oil Cooler Housing