For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the passenger side instrument panel molding. Refer to Instrument Panel Molding Replacement - Passenger Side.
2. Remove the driver side instrument panel molding. Refer to Instrument Panel Molding Replacement - Driver Side.

1 | Instrument Panel Upper and Lower Center Trim Panel Fastener (Qty: 6)

#### Procedure

1. Release both I/P center trim panels from the instrument panel and separate the panels.
2. Use a flat-bladed plastic trim tool in order to release the retaining clips securing the I/P upper center trim panel to the instrument panel.
3. Disconnect the electrical connections.

2 | Instrument Panel Upper Center Trim Panel Retainer (Qty: 2)

#### Procedure

Release the I/P upper center trim panel from the I/P lower center trim panel.

3 | Instrument Panel Upper Center Trim Panel

#### Procedure

When replacing the I/P upper center trim panel, transfer all necessary parts.