For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the front side door trim panel. Refer to Front Side Door Trim Panel Replacement
2. Remove the front side door window frame garnish molding. Refer to Front Side Door Window Frame Garnish Molding Replacement

1 | Front Side Door Window Inner Sealing Strip

#### Procedure

Pull the sealing strip up and away from the door flange to remove.