For 1990-2009 cars

## Cylinder Head Installation LDK

#### Special Tools

EN-45059 Angle Meter

For equivalent regional tools, refer to Special Tools.

Note: Do not use any sealing material.

1. Install the cylinder head gasket (2) to the block.
2. Install the cylinder head (1). Ensure the number 1 cylinder is at top dead center (TDC). The key on the crankshaft should be on top in the 12 o'clock position.

Caution: Refer to Fastener Caution in the Preface section.

Note: Always use NEW cylinder head bolts.

3. Install NEW cylinder head bolts.

3.1. | Tighten the bolts in sequence to 30 N·m (22 lb ft).

3.2. | Tighten the bolts an additional 155 degrees in sequence using the EN-45059 angle meter .

4. Install the front cylinder head bolts (1) and tighten to 35 N·m (26 lb ft).