For 1990-2009 cars

## Camshaft Sprocket Installation LLU

#### Special Tools

EN-45059 Angle Sensor Kit

For equivalent regional tools, refer to Special Tools.

Note: 2 mechanics are required.

1. Install the 2 camshaft sprockets (3).
2. Install the 2 camshaft sprocket washer (2) and the 2 camshaft sprocket bolts (1).
3. Tighten the bolts in two passes.

Hold at the appropriate camshaft hexagon.

Caution: Refer to Fastener Caution in the Preface section.

3.1. | First pass tighten to 50 N·m(37 lb ft).

3.2. | Second pass to 60° + 15° using the EN-45059 sensor kit .