For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the steering wheel inflatable restraint module coil. Refer to Steering Wheel Inflatable Restraint Module Coil Replacement.

1 | Steering Angle Sensor

#### Procedure

1. Press in the clip on the inflatable restraint steering wheel module clock-spring coil to remove the sensor.
2. After installation centre the steering angle sensor. Refer to Steering Angle Sensor Centering.