For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
General Data

- Engine Type

4-Cylinder Inline

- Displacement

1.956 L

120 cu in

- Bore

83.0 mm

3.3 in

- Bore Distance

90.0 mm

3.55 in

- Stroke

90.4 mm

3.56 in

- Compression Ratio

16.5:1

- Maximum Power @ Engine Speed kW/RPM

117.3 kW/4000 RPM

- Maximum Torque @ Engine Speed N·m/RPM

350 N·m/1750 RPM

- Idle Speed

850 RPM

- Firing Order

1-3-4-2

- Engine Height - Total Dimensions Oil Pan to Cover

708 mm

28 in

- Engine Length - Mounting Bracket to Thermostat Housing

701 mm

27.6 in

- Engine Width - Include Exhaust and Intake Manifold

611 mm

24 in

- Engine Height - Crank Center to Top

483 mm

19 in

- Engine Length - RFB to Front of Poly V Belt

474.5 mm

18.7 in

- Engine Weight - Opel Format, MT Version

179 kg

395 lb

Block

- Cylinder Block Height

236.5 mm

9.3 in

- Cylinder Bore Diameter

83.0 mm

3.3 in

- Compression Height

46.63 mm

1.84 in

- Conrod Length

145 mm

5.7 in

Engine Oil

- Viscosity

5W30 or 5W40

- Quality

GM-LL-B-025

- Quantity

- Oil Change Including Filter

4.5 l

275 cu in

- Oil Change Excluding Filter

Oil Consumption Liter/1 000 km (Run-in and First 5 000 km) | max. 0.3 l | max. 18.3
Oil Consumption Liter/1 000 km (5 000 km up to 100 000 km) | max. 0.15 l | max. 9.2
Cooling System
Coolant Specification | GM Long-Life Coolant - Specification B040 1065
Capacity |
Flow (Engine Outlet @ 4500 min -1 , Thermostat Fully Open) | 150 l/min
Flow (Radiator @ 4500 min -1 , Thermostat Fully Open) | 110 l/min
Thermostat |
Start to Open | 88°C
Fully Open | 95°C