For 1990-2009 cars

## Driver or Passenger Seat Back Cushion Frame Replacement Driver or Passenger Seat:6-way Hybrid

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Remove the driver or passenger seat. Refer to Driver or Passenger Seat Replacement.
3. Remove the front seat recliner lever. Refer to Driver or Passenger Seat Recliner Lever Replacement.
4. Remove the front seat outer adjuster finish cover. Refer to Driver or Passenger Seat Outer Adjuster Finish Cover Replacement.
5. Remove the driver or passenger seat inner recliner finish cover. Refer to Driver or Passenger Seat Inner Recliner Finish Cover Replacement.
6. Remove the front seat head restraint guide bezel. Refer to Front Seat Head Restraint Guide Bezel Replacement.
7. Remove the front seat head restraint. Refer to Driver or Passenger Seat Head Restraint Replacement.
8. Remove the front seat head restraint adjust rod guide. Refer to Front Seat Head Restraint Adjust Rod Guide Replacement.
9. Remove the front seat back cushion pad. Refer to Front Seat Back Cushion Pad Replacement.
10. Remove the front seat lumbar support. Refer to Front Seat Lumbar Support Replacement.

1 | Front Seat Back Frame Fastener (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 20 N·m (15 lb ft)
2 | Front Seat Back Frame

## Driver or Passenger Seat Back Cushion Frame Replacement Driver or Passenger Seat:4-way Hybrid

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Remove the driver or passenger seat. Refer to Driver or Passenger Seat Replacement.
3. Remove the front seat recliner lever. Refer to Driver or Passenger Seat Recliner Lever Replacement.
4. Remove the front seat outer adjuster finish cover. Refer to Driver or Passenger Seat Outer Adjuster Finish Cover Replacement.
5. Remove the driver or passenger seat inner recliner finish cover. Refer to Driver or Passenger Seat Inner Recliner Finish Cover Replacement.
6. Remove the front seat head restraint guide bezel. Refer to Front Seat Head Restraint Guide Bezel Replacement.
7. Remove the front seat head restraint. Refer to Driver or Passenger Seat Head Restraint Replacement.
8. Remove the front seat head restraint adjust rod guide. Refer to Front Seat Head Restraint Adjust Rod Guide Replacement.
9. Remove the front seat back cushion pad. Refer to Front Seat Back Cushion Pad Replacement.
10. Remove Front Seat Lumbar Support Replacement. Refer to Front Seat Lumbar Support Replacement.

1 | Front Seat Back Frame Fastener (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 20 N·m (15 lb ft)
2 | Front Seat Back Frame