For 1990-2009 cars

### Electronic Parking Brake Control Module Programming and Setup

If the electronic parking brake control module is replaced, the following procedures must be performed:

Refer to Service Programming System (SPS).

#### Calibration with Scan Tool

Perform the Parking Brake Calibration procedure in Module Setup.

#### Calibration without Scan Tool

1. Ignition ON, apply and hold the brake pedal.
2. Push and hold the electric parking brake switch down for 5-6 seconds.
3. Release the electric parking brake switch.
4. Momentarily push the electric parking brake switch down.
5. Remove the EPB fuse and reinstall.
6. Apply the electric parking brake.
7. Release the electric parking brake.