For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Disconnect the battery negative terminal. Refer to Battery Negative Cable Disconnection and Connection
2. Remove the engine cover. Refer to Engine Cover Replacement

Warning: Gasoline or gasoline vapors are highly flammable. A fire could occur if an ignition source is present. Never drain or store gasoline or diesel fuel in an open container, due to the possibility of fire or explosion. Have a dry chemical (Class B) fire extinguisher nearby.

1 | Fuel Injector Fuel Feed Pipe to Fuel Injector Fasteners (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 25 N·m 18 lb ft
2 | Fuel Injector Fuel Feed Pipe to Fuel Rail Fasteners (Qty: 4) Tighten 25 N·m 18 lb ft
3 | Fuel Injector Fuel Feed Pipe (Qty: 4)