For 1990-2009 cars

Checks | Causes
--- | ---
Case Assembly |

• | Inspect for cracked or broken case.

• | Inspect for porosity or damage on the sealing surfaces.

• | Inspect for loose oil cooler line bolts or damaged oil cooler line seals.

• | Inspect for damaged manual shift shaft seal.

• | Inspect for damaged or worn axle seal on the axle shafts.

• | Inspect for plugged vent cap.

• | Inspect for loose drain plug.

Valve Body Cover Assembly |

• | Inspect for damaged or warped valve body cover assembly.

• | Inspect for damaged or improperly installed valve body cover gasket.

• | Inspect for loose valve body cover bolts.

• | Inspect for damaged or improperly installed wire connector hole seal.