For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the propeller shaft. Refer to Propeller Shaft Replacement.

1 | Propeller Shaft Flange Nut Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

Use DT-49048 fixture to hold the flange when tightening.

Tighten
100 N·m (74 lb ft)

#### Special Tools

DT-49048 Holding Fixture

For equivalent regional tools, refer to Special Tools.

2 | Differential Clutch Seal

#### Procedure

Use a new seal. Refer to Rear Output Shaft Seal Replacement.

3 | Propeller Shaft Flange

#### Procedure

Inspect the fluid level. Refer to Rear Axle Lubricant Level Inspection.