For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Turn OFF the ignition.
2. Remove the engine sight shield.
3. Remove the charge air cooler outlet air tube. Refer to Charge Air Cooler Outlet Hose Replacement.

1 | Throttle Body Module Fastener (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 10 N·m (89 lb in)
2 | Throttle Body Module

#### Procedure

Disconnect the wiring harness connector.

3 | Throttle Body Module Gasket