For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the rear compartment lid inner panel trim. Refer to Rear Compartment Lid Inner Panel Trim Replacement.

1 | Rear Compartment Lid Latch Fastener (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 9 N·m (80 lb in)
2 | Rear Compartment Lid Latch

#### Procedure

1. Disconnect the electrical connector.
2. Push the lid latch to the left side and then forward.
3. Pull out the lid latch.