For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the front bumper fascia. Refer to Front Bumper Fascia Replacement.
2. Remove the front bumper fascia center support bracket. Refer to Front Bumper Fascia Center Support Bracket Replacement.
3. Remove the power steering fluid reservoir. Refer to Power Steering Fluid Reservoir Replacement.

1 | Power Steering Fluid Cooler Outlet Hose Clamp
2 | Power Steering Fluid Cooler Inlet Hose Clamp
3 | Power Steering Fluid Cooler Caution: Refer to Using Proper Power Steering Fluid Caution in the Preface section.

#### Procedure

1. Remove the power steering fluid cooler pipes from clips.
2. Fill and bleed the power steering system. Refer to Power Steering System Bleeding.
3. Clean any excess power steering fluid from the vehicle.