For 1990-2009 cars

Callout | Component Name
--- | ---
Warning: Relieve the fuel system pressure before servicing fuel system components in order to reduce the risk of fire and personal injury. After relieving the system pressure, a small amount of fuel may be released when servicing the fuel lines or connections. In order to reduce the chance of personal injury, cover the regulator and the fuel line fittings with a shop towel before disconnecting. This will catch any fuel that may leak out. Place the towel in an approved container when the disconnection is complete.

#### Preliminary Procedures

1. Remove engine appearance cover replacement.
2. Remove the fuel feed intermediate pipe. Refer to Fuel Feed Intermediate Pipe Replacement.
3. Release the fuel feed pipe - metal. Refer to Fuel Feed Pipe Replacement.

1 | Fuel Pump Module Fastener (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 15 N·m (11 lb ft)
2 | Fuel Pump Module

#### Procedure

1. Haul the fuel pump insulator of the fuel pump module.
2. Disconnect the electrical connector.