For 1990-2009 cars

### Diagnostic Instructions

• | Perform the Diagnostic System Check - Vehicle prior to using this diagnostic procedure.

• | Review Strategy Based Diagnosis for an overview of the diagnostic approach.

• | Diagnostic Procedure Instructions provides an overview of each diagnostic category.

### DTC Descriptor

DTC P0219: Engine Overspeed Condition

### Circuit/System Description

This DTC is used to indicate that the engine speed exceeded the fuel cutoff limit in gear. This DTC may set if the transmission is placed in a low gear while driving down a steep grade or traveling at a high speed.

### Conditions for Running the DTC

• | The DTC is valid for manual transmissions only.

• | The engine is running.

• | Ignition voltage is between 10-18 volts.

### Conditions for Setting the DTC

The ECM detects the engine speed is greater than 7,000 RPM for greater than 1 second.

### Action Taken When the DTC Sets

DTC P0219 is a Type A DTC.

### Conditions for Clearing the DTC

DTC P0219 is a Type A DTC.

### Circuit/System Verification

Note: This DTC is used for information only. This DTC does NOT indicate there is a condition with the crank sensor or the engine control module (ECM).

DTC P0219 is an informational DTC.