For 1990-2009 cars

Table 1: | Electronic Suspension Control Module Scan Tool Data Parameters
Table 2: | Electronic Suspension Control Module Scan Tool Output Controls

The electronic suspension control module scan tool data parameters list contains all suspension control-related parameters that are available on the scan tool. The list is arranged in alphabetical order. A given parameter may appear in any one of the data lists.

#### Electronic Suspension Control Module Scan Tool Data Parameters

Parameter | System State | Expected Value | Description
--- | --- | --- | ---
Operating Conditions: Ignition ON
Battery Voltage | -- | 11-14 V | The scan tool displays V. This is the current battery voltage.
Left Front Damper Actuator Command | -- | 290-310 mA | The scan tool displays mA. This is the current applied to the left front damper actuator.
Left Front Vertical Body Acceleration | -- | -0.1 to +0.1 m/s² | The scan tool displays m/s². This is the signal from the left front body acceleration sensor.
Left Front Vertical Wheel Acceleration | -- | -0.1 to +0.1 m/s² | The scan tool displays m/s². This is the signal from the left front wheel acceleration sensor.
Left Rear Damper Actuator Command | -- | 290-310 mA | The scan tool displays mA. This is the current applied to the left rear damper actuator.
Rear Vertical Body Acceleration | -- | -0.1 to +0.1 m/s² | The scan tool displays m/s². This is the signal from the rear body acceleration sensor.
Right Front Damper Actuator Command | -- | 290-310 mA | The scan tool displays mA. This is the current applied to the right front damper actuator.
Right Front Vertical Body Acceleration | -- | -0.1 to +0.1 m/s² | The scan tool displays m/s². This is the signal from the right front body acceleration sensor.
Right Front Vertical Wheel Acceleration | -- | -0.1 to +0.1 m/s² | The scan tool displays m/s². This is the signal from the right front wheel acceleration sensor.
Right Rear Damper Actuator Command | -- | 290-310 mA | The scan tool displays mA. This is the current applied to the right rear damper actuator.
Steering Position Sensor Signal | Steering wheel in straight position | -5 to +5 Degree | The scan tool displays Degree. This is the current position of the steering angle sensor.
Steering wheel turned left until stop | 450-500 Degree
Steering wheel turned right until stop | -500 to -450 Degree
Suspension Position Sensor 5 V Reference | -- | 4.8-5.2 V | The scan tool displays V. This is the current wheel and body acceleration sensors supply voltage.
Suspension System Mode | -- | Normal | The scan tool displays Normal, Comfort or Sport depending on the selected mode.
Comfort mode switch pressed | Comfort
Sport mode switch pressed | Sport
Vehicle Speed | -- | 0 km/h (0 MPH) | The scan tool displays km/h (MPH) depending on the current speed of the vehicle.

#### Electronic Suspension Control Module Scan Tool Output Controls

Output Control | Description
--- | ---
Left Front Damper Actuator | Commands the current applied to the left front damper actuator Increase or Decrease.
Left Rear Damper Actuator | Commands the current applied to the left rear damper actuator Increase or Decrease.
Right Front Damper Actuator | Commands the current applied to the right front damper actuator Increase or Decrease.
Right Rear Damper Actuator | Commands the current applied to the right rear damper actuator Increase or Decrease.
Suspension System Mode | Commands the electronic suspension system Active or Inactive.