For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

Open the service opening from the rear compartment side trim panel in order to expose the tail lamp fasteners.

1 | Tail Lamp Fastener (Qty: 2) Tip Hand tighten the fasteners only.
2 | Tail Lamp Warning: Refer to Halogen Bulb Warning in the Preface section.

#### Procedure

1. Pull the tail lamp assembly rearward.
2. Disconnect the tail lamp electrical connector.