For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the air cleaner assembly. Refer to Air Cleaner Assembly Replacement.

1 | Throttle Valve Assembly Engine Venting Pipe
2 | Throttle Valve Assembly Body Hose
3 | Throttle Valve Assembly Fastener (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 10 N·m (89 lb in)
4 | Throttle Valve Assembly