For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the hood hinge. Refer to Hood Hinge Replacement.

1 | Hood Hinge Fastener (Qty: 2) Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

Mark the location of the hood hinge bracket to the body with a grease pencil to aid in alignment.

Tip
Adjust the hood hinge bracket after replacing, if needed.

Tighten
22 N·m 16.2 lb ft)

2 | Hood Hinge Bracket