For 1990-2009 cars

#### Special Tools

• | EN 46106 Engine Flywheel Holding Tool .

• | EN 45059 Torque Angle Sensor Kit .

For equivalent regional tools, refer to Special Tools.

1. Install the engine flywheel (2).
2. Loosely install the NEW 8 engine flywheel bolts (1).
3. Install the EN 46106 engine flywheel holding tool .

Caution: Refer to Fastener Caution in the Preface section.

4. Tighten the NEW 8 engine flywheel bolts (1) to 30 N·m (22 lb ft).
5. Tighten the NEW 8 engine flywheel bolts an additional 75 degrees using the EN 45059 angle meter .
6. Remove the EN 46106 holder .