For 1990-2009 cars

Callout | Component Name
--- | ---
Warning: Refer to SIR Warning in the Preface section.

#### Preliminary Procedures

1. Disable the SIR system. Refer to SIR Disabling and Enabling.
2. Remove the front and rear side door sill trim plate. Refer to Front and Rear Side Door Sill Trim Plate Replacement.

1 | Inflatable Restraint Rear Door Side Impact Sensor Fastener

#### Procedure

1. Release the fastener from the inflatable restraint rear side door impact sensor.
2. Disconnect the electrical connector.

2 | Inflatable Restraint Rear Side Door Impact Sensor

#### Procedure

Push the inflatable restraint rear side door impact sensor upwards and pull it from the B-pillar.