For 1990-2009 cars

## Camshaft Cover Removal LDK

1. Remove the rear lift bracket bolts and rear lift bracket (1).
2. Remove the front lift bracket bolts and front lift bracket (1).
3. Remove the bolt and coil (1).
4. Remove the camshaft housing cover insulator bolts.
5. Remove the camshaft housing cover insulator (1).

Note: The PCV hose should not be disconnected from the camshaft cover as damage to the hose connection will result.

6. Remove the camshaft cover assembly (1).
7. Remove and discard the camshaft cover gasket, camshaft cover grommets, and camshaft cover bolts if they are serviced with the grommets.